	        	 DC Load Flow
	       	------------------

 Tool for solving a DC Load Flow, based on the first half 
iteration of the Fast Decoupled Load Flow in Polar Coordinates
method.

 This tool makes an estimation of the branches power flow on a  
system, by the aproach of a strong active power busbar angulus
coupling. Thereby, branch resistances and shunt suscepatances
are not considered so network losses either.
