Visual Solution Import (VSI):
VSI is a Deep-Editor module that allows the user to display the results obtained by models (popular in Latin)
dispatch, predispatching and hydro-thermal coordination. Although Deep-Editor has its own coordinator hydro-
thermal modules, economic dispatch and Unit Commitment, the Deep-Editor interface allows users to display 
results from other dispatch software. This tool is called Visual Solution Import (or importer and external 
solutions display). 

In order for VSI to work, there are two important requirements:
1. A Schematic file "coordinated" with the results of external software. That is, one containing schematic 
lines, busbars, generators, loads with (exactly) same nomenclature used by the external software. This process 
MUST be done by the user before using this tool!!! Deep-Editor DOES NOT automatically builds a schematic from 
the results of other software because the visual arrangement of elements in a unilinear necessarily require 
user participation. CE-FCFM can prepare schematics coordinated with these software on request.
2. Output files (result files) for the supported external software: Generally, Deep-Editor expects the file 
structure / folders / sub-folders WITHOUT any modifications (ie. the results as they were thrown by the external 
software, without any modifications).

Data can be read from two different data sources:
1. Local Folder: Reading files from local source. That is, the Deep-Editor will search the output files in a
local address. The files, which are usually written in csv text format (industry standard), will be read from 
the local disk and loaded into the schematic.
2. Reading Output from Database: In this case, the Deep-Editor would connect to a database (MySQL or MS Access) 
and extract the required dispatch information (results from external software). The format of this database is 
specific and requires the information in tables. EC-FCFM has an information system with test cases. 

More details on the DEEP-EDITOR MANUAL