	        Java Load Flow
	        --------------------

 Tool for solving an AC Load Flow, based on the Full Newton-
Raphson Load Flow in Polar Coordinates Method.


	        Calculus Parameters:

 * "Use of Constant Jacobian Matrix": Setting this flag allows
 to reduce the computing total time of calculus in Large Systems
 by no recaluation and retriangularization of the Load Flow
 Jacobian Matrix. However, when the convergence could be 
 compromissed this setting will be ingnored.

 * "Adjust to Satisfy Q limits Generation": this option set on or
 off the verifying of Reactive Power Generation in "PV" 
 Generators are between their limits and the needed 
 adjustements when a violation take place. An off flag could
 help to find a solution when the Q limits constrains causes a
 no-convergence.

 * "Include Convergence Report on Output File": This report
 contain information about convergence patern and relevant 
 events during calculation. Set on the flag if you want see it. 
